~pageId("devcfg")~~inc:header.inc~
Device IO Configuration - ~label~
~postDevIOconfig~

# Device IO Configuration

This page allows the configuration of the WiSteer device's inputs/outputs settings.

ERROR: A field was unparsable or too much data was POSTed. Try again.

CAUTION: Incorrect settings may cause the device to lose network connectivity. Recovery options will be provided on the next page.

Enter the new settings for the device below:

~inc:images/cmds/imglst.inc~
Main settings ~if formConfigured("configMain")~ ~endif~
WiSteer label:
WiSteer mode:
Protect all pages with password
Show activity panel on home page
Enable boost mode
Browse network for other wisteer devices
Allow propagation of MPFS upload
Enable Activity leds
Halt on fatal errors
Enable DEBUG information
Enable TEST mode (theme colors changed)
~if wisteerMpfsDynamic~
MPFS upload enabled
~endif~
WiSteer login:
Password:
Retype password:
GPS coordinates:

Latitude: |  | Longitude: |  |

GPS distance:

Distance max (km): |  |

~if category_available~
~while cfg_catMainEnum~
- Category ~cfg_catMainEnumNo~:
~wend~ ~endif~
Time settings ~if formConfigured("configTime")~ ~endif~
Synchronize with time server
(~timeScanStart~)
Time:

|  |  |  |  |  |  | : |  | : |

Time server:
Time zone:
Time Bias:
Daylight saving time
Daylight Date:

|  |  |  |  |  |  | : |  | : |

Daylight Bias:
Standard Date:

|  |  |  |  |  |  | : |  | : |

Standard Bias:
Commands settings ~if formConfigured("configCmds")~ ~endif~
Commands:
~while cfg_cmdCfgEnum~
- Command ~cfg_cmdCfgEnumId~:
Image:
Display priority:
~if category_available~ ~while cfg_cmdCfgEnumCatEnum~
- Category ~cfg_cmdCfgEnumCatEnumNo~:
~wend~ ~endif~
Command type:
~if cfg_cmdCfgEnumTypeIs(1)~
Output pin:
Output type:
~if cfg_cmdCfgEnumIOtypeIs(1)~
Reverse action:
ON duration:
~elseif cfg_cmdCfgEnumIOtypeIs(5)~
OFF action:
ON duration:
~elseif cfg_cmdCfgEnumIOtypeIs(6)~
ON action:
~elseif cfg_cmdCfgEnumIOtypeIs(2)~
ON pulse duration:
OFF action:
Input pin for ON status:
Input pin for OFF status:
Input pin for Running status:
~elseif cfg_cmdCfgEnumIOtypeIs(3)~
OFF pulse duration:
ON action:
Input pin for ON status:
Input pin for OFF status:
Input pin for Running status:
~elseif cfg_cmdCfgEnumIOtypeIs(4)~
Pulse duration:
Input pin for ON status:
Input pin for OFF status:
Input pin for Running status:
~endif~
Time before next command:
~elseif cfg_cmdCfgEnumTypeIs(2)~
Input pin:
Input type:
~if cfg_cmdCfgEnumIOtypeIs(1)~ ~elseif cfg_cmdCfgEnumIOtypeIs(2)~
ON pulse duration:
Optional input pin 2:
~elseif cfg_cmdCfgEnumIOtypeIs(3)~
OFF pulse duration:
Optional input pin 2:
~elseif cfg_cmdCfgEnumIOtypeIs(4)~
Pulse duration:
Optional input pin 2:
~endif~
Input action:
~elseif cfg_cmdCfgEnumTypeIs(3)~
Link type:
Link action:
~endif~
User confirmation:
~wend~
IO settings ~if formConfigured("configIOs")~ ~endif~
Inputs/Outputs:
~while cfg_ioEnum~
- :
Pin type:
~if cfg_ioEnumTypeIs(4)~
Dimmer:
~endif~
~wend~
Categories ~if formConfigured("configCats")~ ~endif~
Categories:
~while cfg_catEnum~
- Category ~cfg_catEnumId~:
~wend~
WiSteer tools: ~if deviceLinked~ ~endif~
~inc:footer.inc~