Images used: 
Wisteer "logo" icon/favicon: 
	https://www.iconfinder.com/icons/88531/control_panel_icon#size=128
Up/Down arrows:
	https://www.iconfinder.com/icons/9185/arrow_down_icon#size=16
	https://www.iconfinder.com/icons/9191/arrow_up_icon#size=16

https://www.iconfinder.com/icons/86868/portal_icon#size=128
https://www.iconfinder.com/icons/86867/portal_icon#size=128
https://www.iconfinder.com/icons/18010/bushes_door_home_house_parcel_windows_icon#size=256
https://www.iconfinder.com/icons/32675/light_power_switch_icon#size=128
https://www.iconfinder.com/icons/49734/bulb_idea_light_icon#size=400	
https://www.iconfinder.com/icons/71005/inactive_lamp_icon#size=32
https://www.iconfinder.com/icons/71004/active_lamp_icon#size=32
https://www.iconfinder.com/icons/71050/clock_time_icon#size=32	
https://www.iconfinder.com/icons/94156/by_criteria_data_filter_stock_icon#size=24
https://www.iconfinder.com/icons/18222/monitor_options_screen_settings_icon#size=24
https://www.iconfinder.com/icons/23505/magnifier_original_search_zoom_icon#size=24
https://www.iconfinder.com/icons/62149/arrow_circle_left_refresh_reload_icon#size=24
https://www.iconfinder.com/icons/314692/icon_lock_icon#size=32
https://www.iconfinder.com/icons/314697/icon_lock_open_rounded_icon#size=32
https://www.iconfinder.com/icons/71024/button_off_radio_icon#size=32	
Config	
   CMD types:
	-> Label
	-> Display priority
	-> Categories
   Output/
        -> Pin O: Relay1,2,3,4, IO1,2,3,4,5,6
		-> Output type:
			Relay switch
				-> Cmd INV : (inputs excluded) or Category output: ...
			Relay push ON
				-> Pulse duration: 50ms/100ms/200/300 ... 5minutes
				-> Cmd OFF : (inputs excluded) or Category output: ...
			Relay push OFF
				-> Pulse duration: 50ms/100ms/200/300 ... 5minutes
				-> Cmd ON : (inputs excluded) or Category output: ...
			Relay push ON/OFF
				-> Pulse duration: 50ms/100ms/200/300 ... 5minutes
   Input/
        -> Pin I: IO1,2,3,4,5,6
		-> Cmd(inputs excluded) or Category output: ...
		-> Button type:
			Switch button
			Push button ON
				-> Pulse duration: 50ms/100ms/200/300 ... 5secondes
			Push button OFF
				-> Pulse duration: 50ms/100ms/200/300 ... 5secondes
			Push button ON/OFF
				-> Pulse duration: 50ms/100ms/200/300 ... 5secondes
   Command/
		-> Cmd(inputs excluded) or Category output: ...
		-> Command type:
			Switch ON
			Switch OFF
			Pulse


 IO types
 Relay1,2,3,4, IO1,2,3,4,5,6
 -> label: 
 -> enabled: ON/OFF 
 -> type: I/O
 -> status: 1/0 